**Wireline**

**Available Services:**

Currently we have a team with which we can perform services of:

* Pipeline Check.
* Mechanical check.
* Zone Change.
* Cleaning: Removal of paraffins, sand and scale through the use of cutters, brushes, sand pumps or hydrostatic or acid pumps.
* Redesign of valves for artificial gas lift and/or blind valves.
* Temperature (BHT) and Background Pressure (BHP) Recording Take: With elements of 0-600 oF and 0-10000 psi.
* Placement of test tool or stopper for packing settlement.
* Opening and closing of shirts for verification of the settlement of the packings.
* Tool Fishing and Guayas: Using fine guaya.
* Single Shot and Multi Shot Fishing: In directional registers.
* Fishing for Detonador Strips.
* Fishing surface valves and safety caps.
* Open pit profiling:
* Induction
* Spontaneous Potential
* Gamma Ray
* Resistivity
* Density – Neutron.
* Sonic.
* Caliper.
* Well-to-hole drilling:
* Plt.
* CBL - VDL Cementing Records.
* Cannonwork.